##### Did You Know?

The statistics for Manual Material Handling (MMH) injuries and accidents report over 600,000 overexertion injuries, comprising 27% of lost workdays. Lifting injuries constitute 370,000 injuries, pushing and pulling injuries constituted 93,000 injuries. There are numerous injuries from strains and sprains, fractures, cuts, and bruises.

##### Prevention:

Good planning and safety practices for handling large loads include the following:

* Get assistance when handling large loads.
* To block a raised load, ensure your hands are not under the load prior to releasing.
* Use blocking materials with proper strength.
* Perform a visual check on edges for cracks, splintered pieces, rounded corners, and other damage.
* Where practical, attach handles or holders to assist with moving loads.
* Use appropriate Personal Protective Equipment (i.e. gloves, safety glass, safety boots, etc.).
* When possible, avoid manual lifting.
* Ensure you understand equipment rating capacity.
* Keep load close to your body.
* Do not bend or twist sideways.

Proper forklift use:

* Center load.
* Don’t overload forklift.
* Travel at the lowest possible position.
* Don’t counterbalance by adding additional weight.

Stacked loads:

* Ensure stacked loads are correctly piled and cross-tiered.
* Ensure areas are free of accumulated materials.
* Do not store materials within 6 feet of hoist ways or 10 feet of exterior walls.
* Properly store incompatible materials separately

Lumber and Brick Storage:

* Maximum stack height of lumber is 16 feet with manual handling and 20 feet with a forklift.
* Ensure no nails or other protruding hazards are in the wood.
* Bricks should be stacked no higher than 7 feet.
* Stacks above 4 feet must taper to 2 inches per foot.

Block and Bag Storage

* Masonry blocks above 6 feet are to be tapered 2 blocks per tier.
* Bags and bundles should have interlocking rows.
	+ There should be a step back at least every 10 layers.
	+ Remove block or bag from the top of the stack.
	+ Baled paper should be at least 10 inches from walls, ceilings or sprinkler heads.

Box and Drum Storage

* Hold boxed material in place with cross ties or shrink wrap.
* Stack drums, barrels or kegs symmetrically (for side storage block the bottom to prevent rolling).
* Use bins or shelves for materials that are not stackable.

Hand Trucks

* Tip the load forward and slip the tongue under the load.
* Maintain a low center of gravity.
* Keep load height low enough to see where you are going.

The information in this document was obtained from sources which, to the best of the writer’s knowledge, are authentic and reliable. Arthur J. Gallagher & Co. makes no guarantee of results and assumes no liability in connection with either the information or recommendations obtained in this document. Moreover, it cannot be assumed that every acceptable procedure is included in this document or that abnormal or unusual circumstances may not warrant or require further or additional procedures.